**Backlight keyboard manual**

         Keys: 110 pcs including 5 programmable keys for gaming

         Ultra durable laser carved key cap

         Keyboard dimension: 51.5\*20\*2.72cm

         Win2000,Win XP, Win ME, Vista,Win7,Win8,Android,linux

1.    Choose LED colors: Three kinds of LED light colors for choice. （Red, blue, green）. Press the R/G/B key choose LED light.

2.    Free driver can manually recording. Maximum each macro recording 10

Byte press "Rec" button to start recording, indicating LED <CAPS/NUMLOCK/SCROLL> slow flash, then G1.

Specifies the recording indicator LED flash, press the button for the effective recording, the recording time is 30S, overtime or beyond words

Section, automatically exit recording, or recording is complete press "Rec" button to exit the recording. Exit all indicator LED restore the current state.

3.    EL-INTENSITY Electro Luminescence:

         FN+PGUP--Brightness increases

         FN+PGUP--Brightness decrease

         The default maximum backlight brightness, brightness / medium light / low light / off, brightness adjustment function fourth gear.

4.    Backlit breathing speed control: backlit by the FN + "-" / FN + "+" control breathing rate, FN + "-". Slow breathing rate, FN + "+" accelerated breathing rate, built-in 10 files, the default 1st gear, 1st gear is 3 second one respiratory cycle, each adding a slow one file each respiratory cycle duration. <Example: The second tranche of two cycles 6 seconds breathing>

5. Increasing FN + Q keys to adjust the key retransmission rate, 2 files, Default settings for the PC, the second tranche of speed 1s/60 bytes.

6. This product supports with EEPROM / no EEPROM function, no EEPROM no macro recording, re-power all keyboard settings to Default. Keypad with EEPROM save all the settings.

7. Press FN + "Rec" button 3S, Clear EEPROM macro recording all information back to the Default state, Backlight LED flash 3S exit

8. FN Combined function：

     FN+F1= Media Sel

     FN+F2= Volume-

     FN+F3= Volume+

     FN+F4= Mute

     FN+F5= CD Stop

     FN+F6= Prev Track

     FN+F7= Play/Pause

     FN+F8= Next Track

     FN+F9= Email

     FN+F10= Web/Home

     FN + F11 = Lock keypad

     FN + F12 = Calculator

     FN + Q = key retransmission rate

     FN + "-" / FN + "=" = control backlight breathing rate

     FN + W = W S A D with interchangeable ↑ ↓ ← →

     FN + LED = light lit -> Backlight breath -> backlight off

     FN + Rec = Clear EEPROM macro recording all information